**Commodore VIC-20: Diagnostics Cable Set – Rev. 0**

**Module Description**

The Diagnostic cable set is one components of the VIC-20 Diagnostics Harness. It consists of four cables:

* The IEC Port Cable (Doc.-No. 159-3-01-\*\*)
* The Control Port Cable (Doc.-No. 159-3-02-\*\*)
* The Cassette Port Cable (Doc.-No. 159-3-03-\*\*)
* The Keyboard RESTORE cable (Doc.-No. 159-3-04-\*\*)

The Keyboard RESTORE cable is attached to the Keyboard PCB (Project-No. 156), a know serves as a strain relief.

The Control Port cable and the Cassette Port cable are both identical to the cables of the C64 diagnostic harness.